Amalfi A




Modular electric deck oven
2 decks composition
Amalfi consists of one or more independent baking chambers and an optional prover or stand. The baking chamber is entirely made of refractory stone with coiled heating elements inside, allowing the perfect heat distribution over the whole surface. This oven is particularly suitable for direct pizza baking, specific for more delicate toppings and recommended for indirect baking on trays. Temperature management is electronic, power control of ceiling and floor is independent. The oven door is hinged at the bottom, with a tempered glass window to check the product during baking. The stand consists of a painted metal structure, while the prover is a stainless steel cabinet equipped with a heating thermostat. The prover can reach the maximum temperature of 149°F, whereas the maximum temperature of the baking chamber is 842°F.
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OPERATION
· Heated by spiral heating elements
· Electronic temperature management with independent adjustment of ceiling
and floor
· Maximum temperature reached 842°F
· Continuous temperatures monitoring in baking chamber by thermocouple
· Vapour ducting using manual butterfly valve

CONSTRUCTION
· Structure made in folded stainless steel
· Side panels in painted sheet metal
· Hood in stainless steel
· Steam duct in stainless steel plate
· Stainless steel door, tempered glass
· Refractory top and side structure
· Dual halogen lighting
· Rock wool heat insulation

ACCESSORIES
· Leavening proofer on wheels height 23 1/2”, 31 1/2”
· Stand with wheels height 23 1/2”, 31 1/2”, 37 1/2”
· Spacer element height 11 13/16”
· Additional tray holder guides for compartment and stand
· Self-condensing hood
· Frontless hood

INTERNAL BAKING DIMENSIONS
Internal height	7”
Internal depth	40 1/2”
Internal widht	25 1/2”
Baking surface	7,5ft2

STANDARD EQUIPMENT
· 20 customisable programs
· Timer
· Economiser
· Independent maximum temperature safety device
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1 baking chamber height 7”
(assembled with stand height 37 1/2”)


[image: ]REAR VIEW	RIGHT SIDE VIEW	FRONT VIEW

NOTE: The dimensions indicated in the views are in inches.

	A
Ø 1/2”
condensate exhaust
	B

fairleads
	D
Ø 5 7/8”
steam exhaust
	E
M6
equipotential screws
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DIMENSIONS
External height 25 5/8” (650mm) External depth	51” (1290mm) External width 40 1/4” (1020mm) Weight		490lb (222kg)

TOTAL BAKING CAPACITY
Tray 26”x18” (600x400)mm	2
Pizza diameter 12”	6
Pizza diameter 18”	2

SHIPPING INFORMATION
Packed in wooden crate
Height	36” (900mm)
Depth	73” (1851mm)
Width	49” (1220mm)
Weight	600lb (272kg)

When	combined	with	leavening compartment or stand:
Max height	73” (1850mm)
Max weight	805lb (365kg)

FEEDING AND POWER
Standard feeding
A.C. V240 3ph
Feeding on request
A.C. V208 3ph
Frequency	60Hz
Max power	7,7kW/DECK
*Average power cons	3,8kWh Ampère max
18,5A/DECK (V240 3ph)
21,4A/DECK (V208 3ph)
Connecting cable for each chamber
9AWG/DECK
Power supply (optional proofer)
A.C. V(208/240) 1ph 60Hz
Max power	1,8kW
*Average power cons	0,9kWh Conn. Cable 14AWG – Ampère 7,5A* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice




REAR VIEW	RIGHT SIDE VIEW	FRONT VIEW
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NOTE: The dimensions indicated in the views are in inches.
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2 baking chambers height 7”
(assembled with proofer height 31 1/2”)
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DIMENSIONS
External height 41 3/8” (1050mm) External depth	51” (1290mm) External width 40 1/4” (1020mm) Weight		834lb (378kg)

TOTAL BAKING CAPACITY
Tray 26”x18” (600x400)mm	4
Pizza diameter 12”	12
Pizza diameter 18”	4

SHIPPING INFORMATION
Packed in wooden crate
Height	51 1/2” (1300mm)
Depth	73” (1851mm)
Width	49” (1220mm)
Weight	966lb (438kg)

When	combined	with	leavening compartment or stand:
Max height	89” (2250mm)
Max weight	1171lb (531kg)

FEEDING AND POWER
Standard feeding
A.C. V240 3ph
Feeding on request
A.C. V208 3ph
Frequency	60Hz
Max power	7,7kW/DECK
*Average power cons	3,8kWh Ampère max
18,5A/DECK (V240 3ph)
21,4A/DECK (V208 3ph)
Connecting cable for each chamber
9AWG/DECK
Power supply (optional proofer)
A.C. V(208/240) 1ph 60Hz
Max power	1,8kW
*Average power cons	0,9kWh Conn. Cable 14AWG – Ampère 7,5A* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice
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NOTE: The dimensions indicated in the views are in inches.
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3 baking chambers height 7”
(assembled with proofer height 23 1/2”)
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DIMENSIONS
External height 57 1/8” (1450mm) External depth		51” (1290mm) External width 40 1/4” (1020mm) Weight	1178lb (534kg)

TOTAL BAKING CAPACITY
Tray 26”x18” (600x400)mm	6
Pizza diameter 12”	18
Pizza diameter 18”	6

SHIPPING INFORMATION
Packed in wooden crate
Height	71”(1800mm)
Depth	73” (1851mm)
Width	49” (1220mm)
Weight	1332lb (604kg)

When	combined	with	leavening compartment or stand:
Max height	109” (2750mm)
Max weight	1537lb (697kg)

FEEDING AND POWER
Standard feeding
A.C. V240 3ph
Feeding on request
A.C. V208 3ph
Frequency	60Hz
Max power	7,7kW/DECK
*Average power cons	3,8kWh Ampère max
18,5A/DECK (V240 3ph)
21,4A/DECK (V208 3ph)
Connecting cable for each chamber
9AWG/DECK
Power supply (optional proofer)
A.C. V(208/240) 1ph 60Hz
Max power	1,8kW
*Average power cons	0,9kWh Conn. Cable 14AWG – Ampère 7,5A* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice
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NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice

Amalfi A
TECHNICAL DATA






	







FEEDING AND POWER
(EACH DECK NEEDS TO BE CONNECTED INDEPENDENTLY AND THE LOAD SHOWN BELOW ARE PER DECK)
	
A.C. V240 3ph 60Hz
	
Standard feeding
	Max power
	kW
	7,7

	
	
	
	*Medium cons/hour
	kWh
	3,8

	
	
	
	Ampère Max
	A/DECK
	18,5

	
	
	
	Connecting cable
	AWG/DECK
	9

	
	
A.C. V208 3ph 60Hz
	
Feeding on request
	Max power
	kW
	7,7

	
	
	
	*Medium cons/hour
	kWh
	3,8

	
	
	
	Ampère Max
	A
	21,7

	
	
	
	Connecting cable
	AWG/DECK
	9

	
	
A.C. V240 3ph 60Hz
boosted heating elements
	
Standard feeding
	Max power
	kW
	10,5

	
	
	
	*Medium cons/hour
	kWh
	5,3

	
	
	
	Ampère Max
	A/DECK
	25,2

	
	
	
	Connecting cable
	AWG/DECK
	9

	
	
A.C. V208 3ph 60Hz
boosted heating elements
	
Feeding on request
	Max power
	kW
	10,5

	
	
	
	*Medium cons/hour
	kWh
	5,3

	
	
	
	Ampère Max
	A/DECK
	29,1

	
	
	
	Connecting cable
	AWG/DECK
	9

	
	
A.C. V(208/240) 1ph 60Hz
	
Proofer
	Max power
	kW
	1,8

	
	
	
	*Medium cons/hour
	kWh
	0,9

	
	
	
	Ampère Max
	A/DECK
	7,5

	
	
	
	Connecting cable
	AWG/DECK
	14
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