


Modular electric deck oven
2 decks composition
Amalfi consists of one or more independent baking chambers and an optional prover or stand. The baking chamber is entirely made of refractory stone with coiled heating elements inside, allowing the perfect heat distribution over the whole surface. This oven is particularly suitable for direct pizza baking, specific for more delicate toppings and recommended for indirect baking on trays. Temperature management is electronic, power control of ceiling and floor is independent. The oven door is hinged at the bottom, with a tempered glass window to check the product during baking. The stand consists of a painted metal structure, while the prover is a stainless steel cabinet equipped with a heating thermostat. The prover can reach the maximum temperature of 149°F, whereas the maximum temperature of the baking chamber is 842°F.
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OPERATION
· Heated by spiral heating elements
· Electronic temperature management with independent adjustment of ceiling
and floor
· Maximum temperature reached 842°F
· Continuous temperatures monitoring in baking chamber by thermocouple
· Vapour ducting using manual butterfly valve

CONSTRUCTION
· Structure made in folded stainless steel
· Side panels in painted sheet metal
· Hood in stainless steel
· Steam duct in stainless steel plate
· Stainless steel door, tempered glass
· Refractory top and side structure
· Dual halogen lighting
· Rock wool heat insulation

ACCESSORIES
· Leavening proofer on wheels height 23 1/2”, 31 1/2”
· Stand with wheels height 23 1/2”, 31 1/2”, 37 1/2”
· Spacer element height 11 13/16”
· Additional tray holder guides for compartment and stand
· Self-condensing hood
· Frontless hood

INTERNAL BAKING DIMENSIONS
Internal height	7”
Internal depth	45 1/4”
Internal widht	43 1/2”
Baking surface	13,8ft2

STANDARD EQUIPMENT
· 20 customisable programs
· Timer
· Economiser
· Independent maximum temperature safety device
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1 baking chamber height 7”
(assembled with stand height 37 1/2”)


REAR VIEW	RIGHT SIDE VIEW	FRONT VIEW
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NOTE: The dimensions indicated in the views are in inches.

	A
Ø 1/2”
condensate exhaust
	B

fairleads
	D
Ø 5 7/8”
steam exhaust
	E
M6
equipotential screws

	
	
	
	




DIMENSIONS
External height	25 5/8” (650mm) External depth		54” (1365mm)
External width	60” (1520mm)
Weight	781lb (354kg)

TOTAL BAKING CAPACITY
Tray 26”x18” (600x400)mm	4
Pizza diameter 12”	12
Pizza diameter 18”	5

SHIPPING INFORMATION
Packed in wooden crate
Height	36” (900mm)
Depth	76” (1930mm)
Width	68” (1720mm)
Weight	891lb (404kg)

When	combined	with	leavening compartment or stand:
Max height	73” (1850mm)
Max weight	1244lb (564kg)

FEEDING AND POWER
Standard feeding
A.C. V240 3ph
Feeding on request
A.C. V208 3ph
Frequency	60Hz
Max power	13,7kW/DECK
*Average power cons	6,9kWh Ampère max
33A/DECK (V240 3ph)
38,1A/DECK (V208 3ph)
Connecting cable for each chamber
7AWG/DECK
Power supply (optional proofer)
A.C. V(208/240) 1ph 60Hz
Max power	1,8kW
*Average power cons	0,9kWh Conn. Cable 14AWG – Ampère 7,5A








* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice



REAR VIEW	RIGHT SIDE VIEW	FRONT VIEW
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NOTE: The dimensions indicated in the views are in inches.

	A
Ø 1/2”
condensate exhaust
	B

fairleads
	D
Ø 5 7/8”
steam exhaust
	E
M6
equipotential screws
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2 baking chambers height 7”
(assembled with proofer height 31 1/2”)
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DIMENSIONS
External height	41 3/8” (1050mm) External depth		54” (1365mm)
External width	60” (1520mm)
Weight	1336lb (606kg)

TOTAL BAKING CAPACITY
Tray 26”x18” (600x400)mm	8
Pizza diameter 12”	24
Pizza diameter 18”	10

SHIPPING INFORMATION
Packed in wooden crate
Height	51 1/2” (1300mm)
Depth	76” (1930mm)
Width	68” (1720mm)
Weight	1160lb (526kg)

When	combined	with	leavening compartment or stand:
Max height	89” (2250mm)
Max weight	1845lb (836kg)

FEEDING AND POWER
Standard feeding
A.C. V240 3ph
Feeding on request
A.C. V208 3ph
Frequency	60Hz
Max power	13,7kW/DECK
*Average power cons	6,9kWh Ampère max
33A/DECK (V240 3ph)
38,1A/DECK (V208 3ph)
Connecting cable for each chamber
7AWG/DECK
Power supply (optional proofer)
A.C. V(208/240) 1ph 60Hz
Max power	1,8kW
*Average power cons	0,9kWh Conn. Cable 14AWG – Ampère 7,5A* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice




3 baking chambers height 7”
(assembled with proofer height 23 1/2”)


[image: ]REAR VIEW	RIGHT SIDE VIEW	FRONT VIEW
NOTE: The dimensions indicated in the views are in inches.
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Ø 1/2”
condensate exhaust
	B

fairleads
	D
Ø 5 7/8”
steam exhaust
	E
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equipotential screws
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DIMENSIONS
External height	57 1/8” (1450mm) External depth		54” (1365mm)
External width	60” (1520mm)
Weight	1892lb (858kg)

TOTAL BAKING CAPACITY
Tray 26”x18” (600x400)mm	12
Pizza diameter 12”	36
Pizza diameter 18”	15

SHIPPING INFORMATION
Packed in wooden crate
Height	71” (1800mm)
Depth	76” (1930mm)
Width	68” (1720mm)
Weight	2046lb (928kg)

When	combined	with	leavening compartment or stand:
Max height	109” (2750mm)
Max weight	2399lb (1088kg)

FEEDING AND POWER
Standard feeding
A.C. V240 3ph
Feeding on request
A.C. V208 3ph
Frequency	60Hz
Max power	13,7kW/DECK
*Average power cons	6,9kWh Ampère max
33A/DECK (V240 3ph)
38,1A/DECK (V208 3ph)
Connecting cable for each chamber
7AWG/DECK
Power supply (optional proofer)
A.C. V(208/240) 1ph 60Hz
Max power	1,8kW
*Average power cons	0,9kWh Conn. Cable 14AWG – Ampère 7,5A* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice



* This value is subject to variation according to the way in which the equipment is used
NOTE: MORETTI FORNI S.P.A. reserves the right to modify the characteristics of the products illustrated in this publication without prior notice

Amalfi D
TECHNICAL DATA








	







FEEDING AND POWER
(EACH DECK NEEDS TO BE CONNECTED INDEPENDENTLY AND THE LOAD SHOWN BELOW ARE PER DECK)
	
A.C. V240 3ph 60Hz
	
Standard feeding
	Max power
	kW
	13,7

	
	
	
	*Medium cons/hour
	kWh
	6,9

	
	
	
	Ampère Max
	A/DECK
	33

	
	
	
	Connecting cable
	AWG/DECK
	7

	
	
A.C. V208 3ph 60Hz
	
Feeding on request
	Max power
	kW
	13,7

	
	
	
	*Medium cons/hour
	kWh
	6,9

	
	
	
	Ampère Max
	A
	38,1

	
	
	
	Connecting cable
	AWG/DECK
	7

	
	
A.C. V240 3ph 60Hz
boosted heating elements
	
Standard feeding
	Max power
	kW
	16,0

	
	
	
	*Medium cons/hour
	kWh
	8,0

	
	
	
	Ampère Max
	A/DECK
	38,5

	
	
	
	Connecting cable
	AWG/DECK
	7

	
	
A.C. V208 3ph 60Hz
boosted heating elements
	
Feeding on request
	Max power
	kW
	16,0

	
	
	
	*Medium cons/hour
	kWh
	8,0

	
	
	
	Ampère Max
	A/DECK
	44,5

	
	
	
	Connecting cable
	AWG/DECK
	7

	
	
A.C. V(208/240) 1ph 60Hz
	
Proofer
	Max power
	kW
	1,8

	
	
	
	*Medium cons/hour
	kWh
	0,9

	
	
	
	Ampère Max
	A/DECK
	7,5

	
	
	
	Connecting cable
	AWG/DECK
	14
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