


MODEL: 	 PROJECT: 	 ITEM #: 	 QTY: 	

	PRODUCT IMAGE		STANDARD FEATURES	
· Heavy-Duty spout with double O-Ring construction and welded

	shoulder for durability
· High precision machining and polished nickel chromium finish
· Color-coded handles
· Optional wrist blade handles available
· Full replacement parts available
· Mounting kit included
· Low Lead Compliance
“L” Models meet California AB-1953 and Vermont S152 standards

	11-400 SHOWN

	
ALSO AVAILABLE IN LOW LEAD BY ADDING “L” TO MODEL NUMBER	




SPECIFICATIONS
· 4” on center deck mount with 1/2” NPT male inlets
· Rough in: Two 7/8” round holes on 4” centers
· Flow rate: 2 GPM max
· Shipping weight: 3 lbs.
· Quantity per case: 20












STANDARD SERIES PLUMBING
4” CENTER DECK MOUNT FAUCETS
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MODEL: 	 PROJECT: 	 ITEM #: 	 QTY: 	

MODELS	
STANDARD SERIES PLUMBING
4” CENTER DECK MOUNT FAUCETS


STANDARD SPOUTS	

	Model Numbers
	Ⓐ
	Ⓑ
	Ⓒ

	11-406
11-412
11-450*
	6”
12”
6”
	1 7/8”
2 5/8”
1 7/8”
	4 3/8”
5 1/8”
4 3/8”


NOTE: Add “L” to end of Model Number for Low Lead Model
*Laundry Faucet includes spout adapter

GOOSENECK SPOUTS	

	Model Numbers
	Ⓓ
	Ⓔ
	Ⓕ

	11-400
	3 1/2”
	5 3/8”
	8”


NOTE: Add “L” to end of Model Number for Low Lead Model
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