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4” Center Deck Mount Faucet with 12” Spout	Royal Series Plumbing



 DESCRIPTION	
· [image: ]4” Center Deck Mount Faucet with 12” Spout, Polished Chrome Finish, 1.8GPM Aerator Installed








11-412L

 STANDARD FEATURES	
· ¼ Turn Ceramic Valves
· Durable Full Range Swing Spout with Double O-Ring Construction
· Lever Handles
· Warranty: 1 Year






 PRODUCT COMPLIANCE	SPECIFICATIONS

Water Inlet
1/2” NPT
Temp. Range
40°F - 180°F
Rough In
7/8” Round Holes on 4” Center
Flow Rate
1.8 GPM
Material
Chrome Plated Brass
Weight
3 lbs.


· [image: ]ASME A112.18.1-2012/CSA B125.1-12
· NSF-61
· NSF/ANSI 372
· Meets ANSI A117.1 (ADA)
· California Proposition 65
· CEC Listed
· Massachusetts Approved
WARNING: Plumbing connections should be made by qualified personnel
who will observe all applicable plumbing, sanitary and safety codes.4
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