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4” Deck Mount Single Lever Faucet with Pop-Up Drain	Silver Series


DESCRIPTION





















PRODUCT COMPLIANCE

· [image: ]NSF-61 & NSF/ANSI 372
· [image: ]ASME A112.18.1-2011/CSA B125.1-11 & NSF/ANSI 372
· Meets ANSI A117.1 (ADA)
· Massachusetts Approved
· CEC Approved
· 
4” Deck Mount Single Lever Faucet with Pop-Up Drain, Polished Chrome Finish,
0.5 GPM Male Aerator Installed, 1.5 GPM Aerator Included


STANDARD FEATURES

· Ceramic cartridge valve
· All metal constuction pop-up drain included
· Single lever handle
· Red/blue color indicator
· Warranty: 1 yearSPECIFICATIONS

Water Inlet
1/2” NPS Male w/ Copper Tubing
Temp. Range
40°F - 180°F
Pressure
20-120 PSI
Rough In
7/8” Round Holes on 4” Center
Flow Rate
0.5 GPM
Material
Brass Underbody
Finish
Polished Chrome
Weight
2.5 lbs.
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WARNING: Plumbing connections should be made by qualified personnel who will observe all applicable plumbing, sanitary and safety codes. California Proposition 65 Warning
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