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· Electrical heating
· Automatic boiler water supply
· Automatic stopping of electric resistances in case of lack of water in the boiler
· Vibration pump
· Stainless steel AISI 304 body
· No water connection neededSPECIFICATIONS
BZ19SPM1IL2 (BZ09)
LL18SPM1IL2 (BZ10)

· 
Steam and hot water brewing through steam wand with lever tap
· Coffee temperature adjustable by inner thermostat
· Coffee pressure gauge
· Water tank and vibration pump
· Stainless steel AISI 304 body
· No water connection needed

SEMI PROFESSIONAL ESPRESSO  COFFEE  MACHINES
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Voltage
110V /50-60 Hz
Power
1,200W
Boiler
1.5 Liters (0.4 gal.)
Tank
3 Liters (0.8 gal.)
Product Dimensions
9.84” (A) x 16.7” (B) x 14.7” (C)
Net weight
42 lbs
Shipping Dimensions
21” (A) x 16” (B) x 18” (C)
Gross weight
48.5 lbs
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BEZZERA

MACCHINE PER CAFFE’ ESPRESSO DAL 1901
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