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GRA-123

Important NOTES:
· Operate at room temperature between 75 - 90° F (24 and 32° C).
· Clearance of 8" required on all sides.
· Mixture must maintain a sugar content between 12 -14%; a lower concentration could seriously damage the mixing parts and gear motors.



· High-performance equipment, for slushes, sherbets and other frozen products
· Double mixing system prevents ice accumulation, for optimum product's consistency
· Cold light illumination with LED
· Stainless steel base: front, side, and rear
· Adjustable consistency
· Safety Stop System
· Air cooling system - Refrigerant Gas R404a
· Manual control keypad
· All models are certifi ed NSF-6 safe for milk










	


	
*Also available in special voltage 220V / 60-50 Hz
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