










































[image: ][image: ]STANDARD FEATURES
· Three group automatic espresso machine with 1-6 cup simultaneous delivery capacity
· Volumetric touchpad with programmable dosages
· Automatic	back-flush	cleaning program per group
· Independent Continuous button for semi-automatic operation
· Two Stainless Steel Swivel Steam jets
· One Stainless Steel hot water jet
· Classic thermal brewing group with dynamic pre-infusion ensures optimal espresso extraction
· Certified ETL, NSF

Optional
· Available Colors: Black, Red, White
· Deep Drip Tray to Accommodate Large Take Out Cups
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	BREW DEVICE
	CUPS PER GROUP
	W x D x H
	BOILER CAPACITY
(liters)
	V.
	AMP.
	P.H.
	Hz
	WATTS
	WEIGHT
(Kg./Lbs.)
	SHIPPING WEIGHT
(Kg./Lbs.)
	INCOMING H2O
	DRAIN
	MIN/MAX
bar

	3
	6
	38 x 22.5 x 22.5
	21
	220
	21
	1
	60
	4600
	85/185
	91/200
	3/8” MALE
	9mm INTERNAL
	2 / 5





[image: ]Rosito Bisani Imports, Inc.
940 South La Brea Avenue, Los Angeles CA, 90036
Tel: 323-937-1888 • Fax: 323-938-0728 • Toll Free: 1-800-848-4444
E-mail: sales@rosito-bisani.com
www.rosito-bisani.com
530 South Henderson Road, Suite F, King of Prussia PA, 19406 Tel: 610-265-5950 • Fax: 888-576-8524
Rosito and Bisani Imports reserve the right to make changes in design specifications and/or to make additional improvements in it’s products without imposing any obligations upon itself to install them on products previously manufactured. © 2013.
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